HCT-TS V1.0.14:
 The pi11 pin is modified to the pull-up state.
HCT-TS V1.0.13:
 1.[TSECL-238]: HCT-TS: If Gyro is not present (R5) is not soldered, Angle monitoring can still be chosen
 2.[TSECL-232]: HCT-TS: Detection of Gyro present/absent and activation/deactivation of Angle functionality

HCT-TS V1.0.12:
 1.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
 2.[TSECL-226]: HCT-TS: BLE: History content should be preset with 0 if history is empty
 3.[TSECL-227]: HCT-TS: Peak Torque value is higher than the ActualTorque when increasing the load
 4.[TSECL-228]: HCT-TS: BLE: Device Access Synchronization is not reset after setting up a torque triggering mode on TS -> App remains blocked
 5.[TSECL-229]: HCT-TS: BLE: DeviceMeasurementControl.Behavior: Flags for continuing with SEND and TORQUE are not considered
 6.[TSECL-230]: HCT-TS: BLE: DeviceMeasurementControl.StartCondition is not considered
 7.[TSECL-232]: HCT-TS: Detection of Gyro present/absent and activation/deactivation of Angle functionality
 8.[TSECL-236]: HCT-TS: BLE: History with missing and duplicate entries when reading out by APP
 9.[TSECL-237]: HCT-TS: BLE: Slow advertising intervall is too fast

HCT-TS V1.0.11:
 1.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
 2.[TSECL-220]: HCT-TS: Settings:Measurement: When increasing and decreasing the values display is not refreshing
 3.[TSECL-222]: HCT-TS: Settings::Measurement::Repetition is wrongly displayed.
 4.[TSECL-223]: HCT-TS: Live Values are not correctly refreshed when a measuremente is performed.

HCT-TS V1.0.10:
 1.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 2.[TSECL-184]: HCT-TS: History details: Angle measurements don't display the "Torque Result".
 3.[TSECL-186]: HCT-TS: Feedback response by button pressing is slow
 4.[TSECL-190]: HCT-TS: Screwcase details: Workflow information is displayed twice
 5.[TSECL-196]: HCT-TS: BLE: Reading the History entry via ID
 6.[TSECL-209]: Workflow: Bug by selecting screwcases
 7.[TSECL-210]: HCT-TS: Name of the Screw Case is not shown and not taken over in history if MeasurementCaseID is 0
 8.[TSECL-211]: Overload: Show Last Measurement screen
 9.[TSECL-212]: HCT-TS050: Buzzer must be activated after "Calibration Required" Torque is achieved
10.[TSECL-214]: HCT-TS: Order of screwcases in workflow incorrect.
11.[TSECL-215]: HCT-TS: Workflow: Wrong display message while adding more than 10 screwcases to a workflow.
12.[TSECL-216]: HCT-TS: Deleting screwcase in workflow removes wrong entry.
13.[TSECL-217]: HCT-TS: Repetition flag is inverted
14.[TSECL-218]: HCT-TS: Workflow - Measurement Case Config returns the wrong screwcase

HCT-TS V1.0.9:
 1.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 2.[TSECL-125]: HCT-TS: .csv File data not correctly saved
 3.[TSECL-166]: HCT-TS: Measurement result is saved incorrectly in History
 4.[TSECL-171]: HCT-TS: It is possible to set a target value outside the calibrated range
 5.[TSECL-176]: HCT-TS: Standby time not working
 6.[TSECL-181]: HCT-TS: Mode >> Settings >> Measurement >> Repetition: OFF does not work
 7.[TSECL-182]: HCT-TS: History entries: Bug by selecting an entry
 8.[TSECL-183]: HCT-TS: Center Screw case name position when "Repeat screw case" screen is displayed
 9.[TSECL-184]: HCT-TS: History details: Angle measurements don't display the "Torque Result".
10.[TSECL-188]: HCT-TS: Stand-by and Dimming time don't work correctly
11.[TSECL-189]: HCT-TS: Update Translation Table
12.[TSECL-190]: HCT-TS: Screwcase details: Workflow information is displayed twice
13.[TSECL-191]: HCT-TS: Extend tolerance range
14.[TSECL-192]: HCT-TS: Remove menu-point "Pre-Warning"
15.[TSECL-193]: HCT-TS: New overload value definition
16.[TSECL-194]: HCT-TS: Live values are are zero
17.[TSECL-195]: HCT-TS: After FW Download of 1.0.8. to Test sample HCT-TS500 Tare is not sucessfully
18.[TSECL-196]: HCT-TS: BLE: Reading the History entry via ID
19.[TSECL-199]: HCT-TS: BLE: Standby time and Dimming time cannot be switched OFF via BLE
20.[TSECL-200]: HCT-TS: FW update via BLE does not work because BLE-controler is not set in Bootloader mode
21.[TSECL-201]: HCT-TS: Adjustable Buzzer noise level
22.[TSECL-202]: HCT-TS: Reduce shown information when selecting a screwcase for a workflow
23.[TSECL-203]: HCT-TS: BLE: History: Year must be between 2020 and 9999
24.[TSECL-204]: HCT-TS: Advertising: Toggle Identification Flags for Quick connect with e.g. mobile App by usage of Down-Button
25.[TSECL-205]: HCT-TS: Activation of a Measurement Case or Workflow should also be possible with MEASUREMENT_START_CONDITION_ACTIVATE

HCT-TS V1.0.8:
 1.[TSECL-180]: HCT-TS: BLE: Workflow Active Position in Meas. Control after asking for Repetition is wrong
 2.[TSECL-178]: HCT-TS: Evaluation time is too long
 3.[TSECL-176]: HCT-TS: Standby time not working
 4.[TSECL-175]: HCT-TS: BLE: Continue by Torque if result Ok/Nok turned on does not work as expected - new torque to start measurement does not work
 5.[TSECL-173]: HCT-TS: BLE: Reading the last history entry does not work
 6.[TSECL-171]: HCT-TS: It is possible to set a target value outside the calibrated range
 7.[TSECL-161]: HCT-TS050: Resolution of Live values and Peak values in not correct when unit selected is "cNm"
 8.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
 9.[TSECL-141]: HCT-TS: BLE: No Continue by Send if result Ok/Nok turned on does not work as expected
10.[TSECL-120]: HCT-TS: Charging indication when TS is turned OFF and charged via USB-cable
11.[TSECL-112]: HCT-TS: Wrong colors and fonts 

HCT-TS V1.0.7:
 1.[TSECL-93]: HCT-TS: BLE: Response_threshold & evaluation_threshold are not considered
 2.[TSECL-119]: HCT-TS: Update Rate of live values is too slow
 3.[TSECL-120]: HCT-TS: Charging indication when TS is turned OFF and charged via USB-cable
 4.[TSECL-144]: HCT-TS: "Peak" und Target" on main screen not left-aligned.
 5.[TSECL-146]: HCT-TS: Display flashes once quickly when switching on and off 
 6.[TSECL-148]: HCT-TS: Screwcase PW-black screen after measurement
 7.[TSECL-153]: HCT-TS: BLE: DeviceMeasurementCaseConfiguration cannot be written to HCT-TS050
 8.[TSECL-156]: HCT-TS: Battery Charging symbol
 9.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
10.[TSECL-163]: HCT-TS: Hide Header-Line on Mainscreen during measurement/operation and show max. reached Peak-value instead
11.[TSECL-173]: HCT-TS: BLE: Reading the last history entry does not work
12.[TSECL-174]: HCT-TS: Angle measurement drifts despite there is no rotation.

HCT-TS V1.0.6:
 1.[TSECL-93]: HCT-TS: BLE: Response_threshold & evaluation_threshold are not considered
 2.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 3.[TSECL-109]: HCT-TS: BLE: Connection Configuration: connection_type: Should be APP HID (3) if App and HID are switched on.
 4.[TSECL-119]: HCT-TS: Update Rate of live values is too slow
 5.[TSECL-134]: HCT-TS: Angle mode: Measurement result is wrong displayed
 6.[TSECL-140]: HCT-TS: BLE: Device Measurement Result - Issues with measurement status flags
 7.[TSECL-141]: HCT-TS: BLE: Device Measurement Configuration - Behavior - No continue by Send if result Ok/Nok turned on does not work as expected
 8.[TSECL-143]: HCT-TS: BLE: Inconsistent transmission of live values via serial interface and BLE
 9.[TSECL-147]: HCT-TS: Settings for Master PW are not saved 
10.[TSECL-148]: HCT-TS: Screwcase PW-black screen after measurement
11.[TSECL-151]: HCT-TS: Tolerances in Angle Mode are not considered correctly, Result is allways NOK
12.[TSECL-152]: HCT-TS: BLE: DeviceMeasurementConfiguration.Behavior: DoNotAskForRepetition is not considered after measurement and evaluation
13.[TSECL-153]: HCT-TS: BLE: DeviceMeasurementCaseConfiguration cannot be written to HCT-TS050
14.[TSECL-154]: HCT-TS: Display backlight LED flicker
15.[TSECL-155]: HCT-TS: Menu>>Connection Screen
16.[TSECL-157]: HCT-TS: Recalibration required symbol
17.[TSECL-159]: HCT-TS: No Measurement, if USB-Cable is connected and history.csv has been opened
18.[TSECL-162]: HCT-TS: Menu>>Settings>>Measurement>>Unit: Bug by displaying units
19.[TSECL-164]: HCT-TS: History does not save measurement results correctly
20.[TSECL-165]: HCT-TS: Torque Indicating: Wrong unit displayed by selection of units in Mode>>Settings>>Measurement>>Unit
21.[TSECL-166]: HCT-TS: Measurement result is saved incorrectly in History
22.[TSECL-168]: HCT-TS: Menu>>Settings>>Display>>Brightness: Limit the selection from 12% to 100%
23.[TSECL-169]: HCT-TS: Angle mode: Bug by configuring angle measurement case with "Nm" and "ft.lb" units

HCT-TS V1.0.5:
 Provide FW HCT_TS_50_Beta,HCT_TS_200_Beta,HCT_TS_500_Beta for parameter restore.(TSECL-132)
 Some issues need to be tested with PCB V1.3 samples.(TSECL-120，TSECL-97)
 1.[TSECL-80]: HCT-TS: Wrong tolerances saved in history
 2.[TSECL-97]: HCT-TS: Implementation of RTC functionality
 3.[TSECL-101]: HCT-TS: Button assignment when display orientation is rotated
 4.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 5.[TSECL-106]: HCT-TS: BLE: After factory reset and switching OFF/ON DeviceConnectionConfiguration.HidKeyboardLayout is DE but should be EN
 6.[TSECL-109]: HCT-TS: BLE: Connection Configuration: connection_type: Should be APP HID (3) if App and HID are switched on.
 7.[TSECL-111]: HCT-TS: Wrong Password. Try again? --> Increase font size
 8.[TSECL-117]: HCT-TS: Torque Indicating: No symbol/icon to indicate direction of rotation of measurement
 9.[TSECL-120]: HCT-TS: Charging indication when TS is turned OFF and charged via USB-cable
10.[TSECL-121]: HCT-TS: Change order of Main menu options
11.[TSECL-122]: HCT-TS: Direction symbol not sharp
12.[TSECL-125]: HCT-TS: .csv File data not correctly saved
13.[TSECL-132]: HCT-TS: Wrong default values after flashing FWv1.0.4
14.[TSECL-133]: HCT-TS: Do not show information on unset parameters in the history details
15.[TSECL-134]: Angle mode: Measurement result is wrong displayed
16.[TSECL-135]: HCT-TS: Arrangement of menu texts not identical
17.[TSECL-136]: HCT-TS: Measurement result: Repeat screwcase: Delete symbol from screen
18.[TSECL-137]: HCT-TS: "cNm" unit is not correctly sent in HID
19.[TSECL-138]: HCT-TS: Increase size of mainscreen icons
20.[TSECL-139]: HCT-TS: BLE: Tolerance Max value for a measurement case is not updated correctly for certain units with relative tolerance
21.[TSECL-140]: HCT-TS: BLE: Device Measurement Result - Issues with measurement status flags
22.[TSECL-142]: HCT-TS: BLE: Workflow Content - Worflow id published after activation is -1 

HCT-TS V1.0.4:
 update eeprom fw to a06(Provide calibration parameters)
 1.[TSECL-82]: HCT-TS: Wrong tolerance wording in History detail view
 2.[TSECL-91]: HCT-TS: Evaluation time seems not to be considered correctly
 3.[TSECL-93]: HCT-TS: BLE: Response_threshold & evaluation_threshold are not considered
 4.[TSECL-101]: HCT-TS: Button assignment when display orientation is rotated
 5.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 6.[TSECL-106]: HCT-TS: BLE: After factory reset and switching OFF/ON DeviceConnectionConfiguration.HidKeyboardLayout is DE but should be EN
 7.[TSECL-107]: HCT-TS: Power OFF Behavior when right button is pressed 
 8.[TSECL-109]: HCT-TS: BLE: Connection Configuration: connection_type: Should be APP HID (3) if App and HID are switched on.
 9.[TSECL-110]: HCT-TS: Main screen rotation by pressing B1(Up) or B4(Down)
10.[TSECL-113]: HCT-TS: Delete Scrollbar in Histroy
11.[TSECL-114]: HCT-TS: Loss of torque accuracy after v1.0.3 has been flashed
12.[TSECL-116]: HCT-TS: Angle measurement not accurate
13.[TSECL-118]: HCT-TS: Torque Triggering: Calibrated range not as specified
14.[TSECL-123]: HCT-TS: Mode>>Torque>>Triggering: Min and Max Tolerance not correctly calculated
15.[TSECL-124]: HCT-TS: Bug by configuration of Target value when unit is "Nm" and "ft.lb"

HCT-TS V1.0.3:
 1.Adjust Zero Program -->Angle threshold Value
 2.Modify GUI (Follow Abstract)
 3.Modify csv file
 4.[TSECL-91]: HCT-TS: Evaluation time seems not to be considered correctly.
 5.[TSECL-99]: HCT-TS: EPROM is not saved
 6.[TSECL-105]: HCT-TS: BLE: After a factory reset, the workflow content in the HCT-Interface is not clean
 7.Completion of bootloader and application programs FW,The PCB version of the first sample requires a reburn FW using ST-LINK (HCT_V1.0.2_All.hex or HCT_V1.0.3_All.hex).

HCT-TS V1.0.2:
 1.Completion of bootloader and application programs FW,The PCB version of the first sample requires a reburn FW using ST-LINK (HCT_V1.0.2_All.hex).
 2.Complete usb msc +cdc functionality.

HCT-TS V1.0.1:
 1.Angle / Torque function can be test.

HCT-TS V1.0.0:
 1.Provide the first version of ts fw (New pcb).
 2.Hardware is still being tested.