HCT-TS V1.0.24:
1.[TSECL-293]: HCT-TS: Replace "Workflow PWD" with "History PWD"
2.[TSECL-298]: HCT-TS: “Workflow” shown in Screwcase details (without any Workflow name)
3.[TSECL-299]: HCT-TS: Bug by History entry details when Bluetooth is disabled

HCT-TS V1.0.23:
1.[TSECL-290]: HCT-TS: Default HID Keyboard is EN
2.[TSECL-293]: HCT-TS: Replace "Workflow PWD" with "History PWD"
3.[TSECL-297]: HCT-TS: Add Screwcase "ID" in History Details

HCT-TS V1.0.22:
Screw Case ID corrupted when editing mode on wrench and change from and to Angle Mode
1.[TSECL-290]: HCT-TS: Default HID Keyboard is EN
2.[TSECL-291]: HCT-TS: Target value for CCW measurement is stored incorrectly in EEPROM
3.[TSECL-292]: HCT-TS: Words in csv-file for language german not spelled correctly
4.[TSECL-293]: HCT-TS: Replace "Workflow PWD" with "History PWD"
5.[TSECL-295]: HCT-TS: Fix the noise issue in the same way as done for v1.0.21BETA

HCT-TS V1.0.21:
When the Bluetooth function is turned off, the serial number displayed on the INFO screen is incorrect.
When Bluetooth is turned off, the order of the menu items on the main options screen is incorrect.

HCT-TS V1.0.20:
1.[TSECL-269]: HCT-TS: Again Problems when reading out history entriese via mobile APP (RACP-Mechanism)
2.[TSECL-274]: HCT-TS: Default HID Keyboard is German

HCT-TS V1.0.19:
1.[TSECL-277]: HCT-TS: Definition of OK Button in main screen
2.[TSECL-276]: HCT-TS: LED-Ring should also blink, when Common Alert is set
3.[TSECL-275]: HCT-TS: Wrong unit (cNm) shown in Angle mode, while snug torque is reached

HCT-TS V1.0.18:
Update i2c speed
eeprom : 100k -> 400k
Angle  : Restore to v1.0.13
Torque : Restore to v1.0.13
 1.[TSECL-269]: HCT-TS: Again Problems when reading out history entriese via mobile APP (RACP-Mechanism)
 2.[TSECL-248]: HCT-TS:BLE: In indicating mode, DeviceMeasurementResult and DeviceMeasurementControl are swaped

HCT-TS V1.0.17:
 1.[TSECL-263]: HCT-TS: BLE: ScanResponse GTIN is not correct
 2.[TSECL-248]: HCT-TS:BLE: In indicating mode, DeviceMeasurementResult and DeviceMeasurementControl are swaped
 3.[TSECL-242]: HCT-TS: HID Keyboard Language Default value
 4.[TSECL-233]: HCT-TS: If history is full, the user should only confirm once
 5.[TSECL-227]: HCT-TS: Peak Torque value is higher than the ActualTorque when increasing the load

HCT-TS V1.0.16:
 1.[TSECL-240]: HCT-TS: Recognition of changed EEPROM Structure by means of Versioning the EEPROM structure

HCT-TS V1.0.15:
 Adjust history storage address, need to run factory reset.
 1.[TSECL-239]: HCT-TS: BLE: Confirmation Timeout is not considered, when "Do not continue by Torque/Send if result Ok/Nok" is set
 2.[TSECL-235]: HCT-TS: History.csv with missing entries when reading out
 3.[TSECL-234]: HCT-TS: BLE: Deletion of an active screw case is not possible
 4.[TSECL-225]: HCT-TS: BLE: After factory reset response threshold is 6 but should be 5
 5.[TSECL-219]: HCT-TS: Workflow - Screw Case Name in the display does not update
 6.[TSECL-160]: HCT-TS: Implementation of Battery status aligment

HCT-TS V1.0.14:
 The pi11 pin is modified to the pull-up state.
HCT-TS V1.0.13:
 1.[TSECL-238]: HCT-TS: If Gyro is not present (R5) is not soldered, Angle monitoring can still be chosen
 2.[TSECL-232]: HCT-TS: Detection of Gyro present/absent and activation/deactivation of Angle functionality

HCT-TS V1.0.12:
 1.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
 2.[TSECL-226]: HCT-TS: BLE: History content should be preset with 0 if history is empty
 3.[TSECL-227]: HCT-TS: Peak Torque value is higher than the ActualTorque when increasing the load
 4.[TSECL-228]: HCT-TS: BLE: Device Access Synchronization is not reset after setting up a torque triggering mode on TS -> App remains blocked
 5.[TSECL-229]: HCT-TS: BLE: DeviceMeasurementControl.Behavior: Flags for continuing with SEND and TORQUE are not considered
 6.[TSECL-230]: HCT-TS: BLE: DeviceMeasurementControl.StartCondition is not considered
 7.[TSECL-232]: HCT-TS: Detection of Gyro present/absent and activation/deactivation of Angle functionality
 8.[TSECL-236]: HCT-TS: BLE: History with missing and duplicate entries when reading out by APP
 9.[TSECL-237]: HCT-TS: BLE: Slow advertising intervall is too fast

HCT-TS V1.0.11:
 1.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
 2.[TSECL-220]: HCT-TS: Settings:Measurement: When increasing and decreasing the values display is not refreshing
 3.[TSECL-222]: HCT-TS: Settings::Measurement::Repetition is wrongly displayed.
 4.[TSECL-223]: HCT-TS: Live Values are not correctly refreshed when a measuremente is performed.

HCT-TS V1.0.10:
 1.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 2.[TSECL-184]: HCT-TS: History details: Angle measurements don't display the "Torque Result".
 3.[TSECL-186]: HCT-TS: Feedback response by button pressing is slow
 4.[TSECL-190]: HCT-TS: Screwcase details: Workflow information is displayed twice
 5.[TSECL-196]: HCT-TS: BLE: Reading the History entry via ID
 6.[TSECL-209]: Workflow: Bug by selecting screwcases
 7.[TSECL-210]: HCT-TS: Name of the Screw Case is not shown and not taken over in history if MeasurementCaseID is 0
 8.[TSECL-211]: Overload: Show Last Measurement screen
 9.[TSECL-212]: HCT-TS050: Buzzer must be activated after "Calibration Required" Torque is achieved
10.[TSECL-214]: HCT-TS: Order of screwcases in workflow incorrect.
11.[TSECL-215]: HCT-TS: Workflow: Wrong display message while adding more than 10 screwcases to a workflow.
12.[TSECL-216]: HCT-TS: Deleting screwcase in workflow removes wrong entry.
13.[TSECL-217]: HCT-TS: Repetition flag is inverted
14.[TSECL-218]: HCT-TS: Workflow - Measurement Case Config returns the wrong screwcase

HCT-TS V1.0.9:
 1.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 2.[TSECL-125]: HCT-TS: .csv File data not correctly saved
 3.[TSECL-166]: HCT-TS: Measurement result is saved incorrectly in History
 4.[TSECL-171]: HCT-TS: It is possible to set a target value outside the calibrated range
 5.[TSECL-176]: HCT-TS: Standby time not working
 6.[TSECL-181]: HCT-TS: Mode >> Settings >> Measurement >> Repetition: OFF does not work
 7.[TSECL-182]: HCT-TS: History entries: Bug by selecting an entry
 8.[TSECL-183]: HCT-TS: Center Screw case name position when "Repeat screw case" screen is displayed
 9.[TSECL-184]: HCT-TS: History details: Angle measurements don't display the "Torque Result".
10.[TSECL-188]: HCT-TS: Stand-by and Dimming time don't work correctly
11.[TSECL-189]: HCT-TS: Update Translation Table
12.[TSECL-190]: HCT-TS: Screwcase details: Workflow information is displayed twice
13.[TSECL-191]: HCT-TS: Extend tolerance range
14.[TSECL-192]: HCT-TS: Remove menu-point "Pre-Warning"
15.[TSECL-193]: HCT-TS: New overload value definition
16.[TSECL-194]: HCT-TS: Live values are are zero
17.[TSECL-195]: HCT-TS: After FW Download of 1.0.8. to Test sample HCT-TS500 Tare is not sucessfully
18.[TSECL-196]: HCT-TS: BLE: Reading the History entry via ID
19.[TSECL-199]: HCT-TS: BLE: Standby time and Dimming time cannot be switched OFF via BLE
20.[TSECL-200]: HCT-TS: FW update via BLE does not work because BLE-controler is not set in Bootloader mode
21.[TSECL-201]: HCT-TS: Adjustable Buzzer noise level
22.[TSECL-202]: HCT-TS: Reduce shown information when selecting a screwcase for a workflow
23.[TSECL-203]: HCT-TS: BLE: History: Year must be between 2020 and 9999
24.[TSECL-204]: HCT-TS: Advertising: Toggle Identification Flags for Quick connect with e.g. mobile App by usage of Down-Button
25.[TSECL-205]: HCT-TS: Activation of a Measurement Case or Workflow should also be possible with MEASUREMENT_START_CONDITION_ACTIVATE

HCT-TS V1.0.8:
 1.[TSECL-180]: HCT-TS: BLE: Workflow Active Position in Meas. Control after asking for Repetition is wrong
 2.[TSECL-178]: HCT-TS: Evaluation time is too long
 3.[TSECL-176]: HCT-TS: Standby time not working
 4.[TSECL-175]: HCT-TS: BLE: Continue by Torque if result Ok/Nok turned on does not work as expected - new torque to start measurement does not work
 5.[TSECL-173]: HCT-TS: BLE: Reading the last history entry does not work
 6.[TSECL-171]: HCT-TS: It is possible to set a target value outside the calibrated range
 7.[TSECL-161]: HCT-TS050: Resolution of Live values and Peak values in not correct when unit selected is "cNm"
 8.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
 9.[TSECL-141]: HCT-TS: BLE: No Continue by Send if result Ok/Nok turned on does not work as expected
10.[TSECL-120]: HCT-TS: Charging indication when TS is turned OFF and charged via USB-cable
11.[TSECL-112]: HCT-TS: Wrong colors and fonts 

HCT-TS V1.0.7:
 1.[TSECL-93]: HCT-TS: BLE: Response_threshold & evaluation_threshold are not considered
 2.[TSECL-119]: HCT-TS: Update Rate of live values is too slow
 3.[TSECL-120]: HCT-TS: Charging indication when TS is turned OFF and charged via USB-cable
 4.[TSECL-144]: HCT-TS: "Peak" und Target" on main screen not left-aligned.
 5.[TSECL-146]: HCT-TS: Display flashes once quickly when switching on and off 
 6.[TSECL-148]: HCT-TS: Screwcase PW-black screen after measurement
 7.[TSECL-153]: HCT-TS: BLE: DeviceMeasurementCaseConfiguration cannot be written to HCT-TS050
 8.[TSECL-156]: HCT-TS: Battery Charging symbol
 9.[TSECL-160]: HCT-TS: Implementation of Battery status aligment
10.[TSECL-163]: HCT-TS: Hide Header-Line on Mainscreen during measurement/operation and show max. reached Peak-value instead
11.[TSECL-173]: HCT-TS: BLE: Reading the last history entry does not work
12.[TSECL-174]: HCT-TS: Angle measurement drifts despite there is no rotation.

HCT-TS V1.0.6:
 1.[TSECL-93]: HCT-TS: BLE: Response_threshold & evaluation_threshold are not considered
 2.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 3.[TSECL-109]: HCT-TS: BLE: Connection Configuration: connection_type: Should be APP HID (3) if App and HID are switched on.
 4.[TSECL-119]: HCT-TS: Update Rate of live values is too slow
 5.[TSECL-134]: HCT-TS: Angle mode: Measurement result is wrong displayed
 6.[TSECL-140]: HCT-TS: BLE: Device Measurement Result - Issues with measurement status flags
 7.[TSECL-141]: HCT-TS: BLE: Device Measurement Configuration - Behavior - No continue by Send if result Ok/Nok turned on does not work as expected
 8.[TSECL-143]: HCT-TS: BLE: Inconsistent transmission of live values via serial interface and BLE
 9.[TSECL-147]: HCT-TS: Settings for Master PW are not saved 
10.[TSECL-148]: HCT-TS: Screwcase PW-black screen after measurement
11.[TSECL-151]: HCT-TS: Tolerances in Angle Mode are not considered correctly, Result is allways NOK
12.[TSECL-152]: HCT-TS: BLE: DeviceMeasurementConfiguration.Behavior: DoNotAskForRepetition is not considered after measurement and evaluation
13.[TSECL-153]: HCT-TS: BLE: DeviceMeasurementCaseConfiguration cannot be written to HCT-TS050
14.[TSECL-154]: HCT-TS: Display backlight LED flicker
15.[TSECL-155]: HCT-TS: Menu>>Connection Screen
16.[TSECL-157]: HCT-TS: Recalibration required symbol
17.[TSECL-159]: HCT-TS: No Measurement, if USB-Cable is connected and history.csv has been opened
18.[TSECL-162]: HCT-TS: Menu>>Settings>>Measurement>>Unit: Bug by displaying units
19.[TSECL-164]: HCT-TS: History does not save measurement results correctly
20.[TSECL-165]: HCT-TS: Torque Indicating: Wrong unit displayed by selection of units in Mode>>Settings>>Measurement>>Unit
21.[TSECL-166]: HCT-TS: Measurement result is saved incorrectly in History
22.[TSECL-168]: HCT-TS: Menu>>Settings>>Display>>Brightness: Limit the selection from 12% to 100%
23.[TSECL-169]: HCT-TS: Angle mode: Bug by configuring angle measurement case with "Nm" and "ft.lb" units

HCT-TS V1.0.5:
 Provide FW HCT_TS_50_Beta,HCT_TS_200_Beta,HCT_TS_500_Beta for parameter restore.(TSECL-132)
 Some issues need to be tested with PCB V1.3 samples.(TSECL-120，TSECL-97)
 1.[TSECL-80]: HCT-TS: Wrong tolerances saved in history
 2.[TSECL-97]: HCT-TS: Implementation of RTC functionality
 3.[TSECL-101]: HCT-TS: Button assignment when display orientation is rotated
 4.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 5.[TSECL-106]: HCT-TS: BLE: After factory reset and switching OFF/ON DeviceConnectionConfiguration.HidKeyboardLayout is DE but should be EN
 6.[TSECL-109]: HCT-TS: BLE: Connection Configuration: connection_type: Should be APP HID (3) if App and HID are switched on.
 7.[TSECL-111]: HCT-TS: Wrong Password. Try again? --> Increase font size
 8.[TSECL-117]: HCT-TS: Torque Indicating: No symbol/icon to indicate direction of rotation of measurement
 9.[TSECL-120]: HCT-TS: Charging indication when TS is turned OFF and charged via USB-cable
10.[TSECL-121]: HCT-TS: Change order of Main menu options
11.[TSECL-122]: HCT-TS: Direction symbol not sharp
12.[TSECL-125]: HCT-TS: .csv File data not correctly saved
13.[TSECL-132]: HCT-TS: Wrong default values after flashing FWv1.0.4
14.[TSECL-133]: HCT-TS: Do not show information on unset parameters in the history details
15.[TSECL-134]: Angle mode: Measurement result is wrong displayed
16.[TSECL-135]: HCT-TS: Arrangement of menu texts not identical
17.[TSECL-136]: HCT-TS: Measurement result: Repeat screwcase: Delete symbol from screen
18.[TSECL-137]: HCT-TS: "cNm" unit is not correctly sent in HID
19.[TSECL-138]: HCT-TS: Increase size of mainscreen icons
20.[TSECL-139]: HCT-TS: BLE: Tolerance Max value for a measurement case is not updated correctly for certain units with relative tolerance
21.[TSECL-140]: HCT-TS: BLE: Device Measurement Result - Issues with measurement status flags
22.[TSECL-142]: HCT-TS: BLE: Workflow Content - Worflow id published after activation is -1 

HCT-TS V1.0.4:
 update eeprom fw to a06(Provide calibration parameters)
 1.[TSECL-82]: HCT-TS: Wrong tolerance wording in History detail view
 2.[TSECL-91]: HCT-TS: Evaluation time seems not to be considered correctly
 3.[TSECL-93]: HCT-TS: BLE: Response_threshold & evaluation_threshold are not considered
 4.[TSECL-101]: HCT-TS: Button assignment when display orientation is rotated
 5.[TSECL-104]: HCT-TS: Improvement of acoustic and haptic feedack
 6.[TSECL-106]: HCT-TS: BLE: After factory reset and switching OFF/ON DeviceConnectionConfiguration.HidKeyboardLayout is DE but should be EN
 7.[TSECL-107]: HCT-TS: Power OFF Behavior when right button is pressed 
 8.[TSECL-109]: HCT-TS: BLE: Connection Configuration: connection_type: Should be APP HID (3) if App and HID are switched on.
 9.[TSECL-110]: HCT-TS: Main screen rotation by pressing B1(Up) or B4(Down)
10.[TSECL-113]: HCT-TS: Delete Scrollbar in Histroy
11.[TSECL-114]: HCT-TS: Loss of torque accuracy after v1.0.3 has been flashed
12.[TSECL-116]: HCT-TS: Angle measurement not accurate
13.[TSECL-118]: HCT-TS: Torque Triggering: Calibrated range not as specified
14.[TSECL-123]: HCT-TS: Mode>>Torque>>Triggering: Min and Max Tolerance not correctly calculated
15.[TSECL-124]: HCT-TS: Bug by configuration of Target value when unit is "Nm" and "ft.lb"

HCT-TS V1.0.3:
 1.Adjust Zero Program -->Angle threshold Value
 2.Modify GUI (Follow Abstract)
 3.Modify csv file
 4.[TSECL-91]: HCT-TS: Evaluation time seems not to be considered correctly.
 5.[TSECL-99]: HCT-TS: EPROM is not saved
 6.[TSECL-105]: HCT-TS: BLE: After a factory reset, the workflow content in the HCT-Interface is not clean
 7.Completion of bootloader and application programs FW,The PCB version of the first sample requires a reburn FW using ST-LINK (HCT_V1.0.2_All.hex or HCT_V1.0.3_All.hex).

HCT-TS V1.0.2:
 1.Completion of bootloader and application programs FW,The PCB version of the first sample requires a reburn FW using ST-LINK (HCT_V1.0.2_All.hex).
 2.Complete usb msc +cdc functionality.

HCT-TS V1.0.1:
 1.Angle / Torque function can be test.

HCT-TS V1.0.0:
 1.Provide the first version of ts fw (New pcb).
 2.Hardware is still being tested.