Holex V1.1.18:
     1.HOLEXTWECL-389 HOLEXTW: Target value in ftlb is manipulated after activation

Holex V1.1.17:
     1.HOLEXTWECL-389 HOLEXTW: Target value in ftlb is manipulated after activation
     2.HOLEXTWECL-395 HOLEXTW: HCT TW-050: After effective length is changed then angle mode does not work.
	
Holex V1.1.16:
     1.HOLEXTWECL-386 Holex TW: Wrong Target Value when activating a measurement case with torque triggering after measuremement case with angle

Holex V1.1.15:
     1.HOLEXTWECL-383 HOLEXTW FW: Constant Notification of "100 Measurements left" screen when measurements lefts are lower than 100.

Holex V1.1.14:
     1.HOLEXTWECL-374 Holex FW: "Measurements left" reset to 0 after FW-Update

Holex V1.1.13:
     1.HOLEXTWECL-378 Holex FW: When HID is deacivated, then Security is still configured with Bonding
     2.HOLEXTWECL-377 Holex FW: When HID has been switched OFF it is activated again after restart.
     3.HOLEXTWECL-374 Holex FW: "Measurements left" reset to 0 after FW-Update
     4.HOLEXTWECL-368 Holex FW: No Reset when switching ON HCT in Connections menu

Holex V1.1.12:
     1.HOLEXTWECL-370 Calibration Intervall does not work
     2.HOLEXTWECL-368 Holex FW: No Reset when switching ON HCT in Connections menu
     3.HOLEXTWECL-366 Holex FW: Holex FW: Worker guidance software shall be able to lock the tool and alarm when false usage
     4.HOLEXTWECL-360 Holex FW: Customer wants to change the calibration intervall.

Holex V1.1.11:
     1.HOLEXTWECL-367 Holex FW: Inkonsistency in Screw-Case Activation Sequence between Garant and Holex
     2.HOLEXTWECL-366 Holex FW: Worker guidance software shall be able to lock the tool and alarm when false usage
     3.HOLEXTWECL-365 Holex FW: Hang Up when activating of measurement cases is too frequent.
     4.HOLEXTWECL-360 Holex FW: Customer wants to change the calibration intervall.

Holex V1.1.10:
     1.HOLEXTWECL-317 Holex TW: All BLE module is deactivated when HID option is deactivated

Holex V1.1.9:
     1.HOLEXTWECL-317 Holex TW: All BLE module is deactivated when HID option is deactivated
     2.HOLEXTWECL-332 Holex TW: Issue when changing units and setpoint at the same time
     
Holex V1.1.8:
     1.HOLEXTWECL-295 Measurement threshold out of range
     2.HOLEXTWECL-317 Holex TW: All BLE module is deactivated when HID option is deactivated
     3.HOLEXTWECL-318 Menu Switch for Repetition
     4.HOLEXTWECL-323 Leave the result screen, when new MeasurementCaseData are activated by APP
     5.HOLEXTWECL-325 HOLEX TW: Tolerance -0,0% and +0,0% as well possible to configure

Holex V1.1.7:
     1.HOLEXTWECL-307 Holex TW: Increase tolerance range from 9,9% to 10,0%
     2.HOLEXTWECL-312 Holex TW: No HID-Value is sent in Triggering Mode, only in Indicating

Holex V1.1.6:
     1.HOLEXTWECL-295 Measurement threshold out of range
     2.HOLEXTWECL-299 HolexTW: If BLE-Module restarts due to a reset, ApplicationFW still shows the BLE-Symbole
     3.HOLEXTWECL-302 Set NumberOfActiveLinks to 1, when HID is switched off
     4.HOLEXTWECL-305 HolexTW: Reduce time between result screens by half

Holex V1.1.5:
     1.HOLEXTWECL-296 HolexTW: StatusQuery after new mode sent by App fails
     2.HOLEXTWECL-298 HolexTW: Sending MeasurementCaseConfiguration data directly after Startup does not activate them.
     3.HOLEXTWECL-299 HolexTW: If BLE-Module restarts due to a reset, ApplicationFW still shows the BLE-Symbole
     4.HOLEXTWECL-301 HOLEX TW: If display is dimmed, display does not switch on when common alert is sent

Holex V1.1.4:
     1.HOLEXTWECL-293 Holex FW: Holex TW: Menu >> Settings >> Measurement >> Threshold: Buzzer and vibration behavior not correct in Torque Triggering and Angle modes 
     2.HOLEXTWECL-294 Holex FW: Holex TW: Menu >> Settings >> Measurement >> Threshold: Modification of Threshold value is not updated for the next measurement, it is updated in the second new measurement.

Holex V1.1.3:
     1.HOLEXTWECL-289 Holex FW: "Overload" state with "Last measured value" screen behaviour

Holex V1.1.2:
     1.HOLEXTWECL-280 No unit in MeasurementCaseConfiguration after StartUp
     2.HOLEXTWECL-282 HOLEX FW: Change wording in screen "Configuration via mobile app"
     3.HOLEXTWECL-287 Holex TW: Alarm when Torque exceeds 125% of maximal load
     4.SW-Trigger for FW-Update over the air.	

Holex V1.1.1:
     1.HOLEXTWECL-270 Holex: Behavior "Do not ask for Repitition" and SequenceCounter cannot be set parallel
     2.HOLEXTWECL-274 Holex TW: Usage Alert: DeviceIoRemoteControl returns AckError 0x0B for INVALID_DATA
     3.HOLEXTWECL-275 HOLEX TW: Small Issue in unblocking of TW

Holex V1.1.0:
     1.HOLEXTWECL-272 Holex: Temporary Unblocking of Wrench
     2.HOLEXTWECL-271 HOLEX: Unblocking does not really work
     3.HOLEXTWECL-270 Holex: Behavior "Do not ask for Repitition" and SequenceCounter cannot be set parallel
     4.HOLEXTWECL-269 Holex: BLE-Version is 0.0.0
     5.HOLEXTWECL-263 Holex TW: BLE-Version in DeviceVersion
     6.HOLEXTWECL-261 Holex TW: Usage Alert
     7.HOLEXTWECL-259 Holex TW: Unblocking of blocked Device
     8.HOLEXTWECL-257 Holex TW HCT-Interface: Option "Do not Ask for Repitition"
     9.HOLEXTWECL-249 HOLEXTW BLE: Advertisement: Behavior of IdentificationFlags
    10.HOLEXTWECL-248 HOLEXTW BLE: Evaluation time (register address:0x00002004) not possible to be set to 1 second 
    11.HOLEXTWECL-243 HOLEXTW FW: Recalibration required message after 5000 measurements
    12.HOLEXTWECL-240 HOLEXTW BLE: Sequence Counter Behavior after not repeated Measurement Case
    13.Update proxy lib to ble_proxy_win_V1.2.16
 
Holex V1.0.6:
    1.HOLEXTWECL-257 Holex TW HCT-Interface: Option "Do not Ask for Repitition"
    2.HOLEXTWECL-259 Holex TW: Unblocking of blocked Device
    3.HOLEXTWECL-261 Holex TW: Usage Alert 
    4.HOLEXTWECL-263 Holex TW: BLE-Version in DeviceVersion

Holex V1.0.5:
    1.HOLEXTWECL-234 HOLEXTW FW: Indicating Mode: Measurement done and "Send" button not pressed.
    2.HOLEXTWECL-237 HOLEXTW BLE: Sending a measurement case with a name
    3.HOLEXTWECL-239 HOLEXTW BLE: Wrong Behavior of Sequence Counter if MeasurementCase fails and user changes MeasurementCase

Holex V1.0.4:
    1.HOLEXTWECL-226 HOLEXTW FW: English Typo: Wrong passord! Try again?
    2.HOLEXTWECL-229 HOLEXTW FW: Menu >> Connection >> Bluetooth = OFF: Wrench firmware frezees after the "Send" button is pressed after no measurement. 
    3.HOLEXTWECL-230 HOLEXTW FW: Menu >> Connection >> HID:ON >> Unit: OFF: It does not work, the unit is still being sended, despite the option is OFF.
    4.HOLEXTWECL-231 HOLEXTW FW: Menu >> Connection >> HID:ON >> Sign: OFF: It does not work, the sign is still being sended, despite the option is OFF.

Holex V1.0.3:
    1.HOLEXTWECL-224 HOLEXTW FW: Angle Mode: Live Angle value is not correctly refreshed after a measurement.
    2.HOLEXTWECL-225 HOLEXTW FW: Angle License issue 

Holex V1.0.2:
    1.HOLEXTWECL-218 HOLEXTW BLE: After switching from an Angle Mode to torque triggering the target value is devided by 10
    2.HOLEXTWECL-217 HOLEXTW FW: Indicating Mode: Direction of rotation is not updated after a change of direction
    3.HOLEXTWECL-214 HOLEXTW FW: Angle Mode: It is possible to configure an screw case with more than 1000°
    4.HOLEXTWECL-213 HOLEXTW FW: Angle Mode: Wrong visualization of result screen and repeat screen when angle measurement is greater than 999,9°

Holex V1.0.1:
    1.HOLEXTWECL-217 HOLEXTW FW: Indicating Mode: Direction of rotation is not updated after a change of direction
    2.HOLEXTWECL-216 HOLEXTW BLE: Mode torque triggering does not show the correct target value
    3.HOLEXTWECL-215 HOLEXTW BLE: Angle Mode Target Angle multiplied by 100

Holex V1.0.0:
    1.HOLEXTWECL-212 HOLEXTW FW: Indicating Mode: Peak Value and Live Value not correct updated when Master PW is enabled
    2.HOLEXTWECL-211 HOLEXTW BLE: Battery Status (Register 0x00000201) is not correctly updated
    3.HOLEXTWECL-210 HOLEXTW FW: Traceability info screen translation
    4.HOLEXTWECL-209 HOLEXTW FW: Master PWD is activated without confirmation of the Password
    5.HOLEXTWECL-208 HOLEXTW FW: French Language: Correct Screen
    6.HOLEXTWECL-207 HOLEXTW FW: Issue when confirming the Master PWD
    7.HOLEXTWECL-206 HOLEXTW BLE: Rounding of target value.
    8.HOLEXTWECL-205 HOLEXTW FW: Spanish Language Typo: "MENÚ", " Crear Contraseña", "Confirmar Contraseña"
    9.HOLEXTWECL-203 HOLEXTW BLE: Measurement Case Data must be resent if in Indicating Mode Measurement Unit is changed.
   10.HOLEXTWECL-201 HOLEXTW BLE: Correct Company prefix in scan response data
   11.HOLEXTWECL-192 HOLEXTW FW: counter for maximal number of measurement actions until recalibration  

Holex V0.2.13:
    1.HOLEXTWECL-203 HOLEXTW BLE: Measurement Case Data must be resent if in Indicating Mode Measurement Unit is changed.
    2.HOLEXTWECL-202 HOLEXTW BLE: The value of the snug torque in measurement case data is not converted to the respective measurement unit
    3.HOLEXTWECL-201 HOLEXTW BLE: Correct Company prefix in scan response data
    4.HOLEXTWECL-200 HOLEXTW FW: Correct screen: Configuration via mobile App
    5.HOLEXTWECL-199 HOLEXTW BLE: Options not write protected
    6.HOLEXTWECL-198 HOLEXTW FW: Correct screen: Overload Info
    7.HOLEXTWECL-197 HOLEXTW FW: Translation Table Update
    8.HOLEXTWECL-196 HOLEXTW FW: Correct Screen: Create Password
    9.HOLEXTWECL-195 HOLEXTW FW: Spanish Language Typo: "Resetear Bluetooth"
   10.HOLEXTWECL-193 HOLEXTW FW: Wrench hangs sometimes if traceability mode is active and closing App
   11.HOLEXTWECL-192 HOLEXTW FW: counter for maximal number of measurement actions until recalibration
   12.HOLEXTWECL-191 HOLEXTW: FW Sequence counter behavior at 999 +1 screw actions
   13.HOLEXTWECL-190 HOLEXTW FW: Upper symbols are not refreshed during a measurement
   14.HOLEXTWECL-189 HOLEXTW FW: Spanish Language Typo: "Recalibración Necesaria"
   15.HOLEXTWECL-186 HOLEXTW FW: Last measured saved
   16.HOLEXTWECL-172 HOLEXTW: Measurement option available Block should be read-only
   17.HOLEXTWECL-157 HOLEXTW FW: "Battery Low" pop-ups screens are not correctly visualized at low voltage

Holex V0.2.12:
    1. HOLEXTWECL-187 HOLEXTW: Torque Triggering Mode cannot be activated from App if no Angle License
    2. HOLEXTWECL-185 HOLEXTW FW: It is possible to unlock the tool by using the App after it was overloaded
    3. HOLEXTWECL-184 HOLEXTW FW: After installation of FW V0.2.11 and startup shut down of TW on prototypes
    4. HOLEXTWECL-183 HOLEXTW FW: Attention Measurement screen does not pop up when the number of measurement left are lower than 500
    5. HOLEXTWECL-162 HOLEXTTW: APP_CONNECTION_ACTIVE_FLAG dissappears once  send button is pressed

Holex V0.2.11:
    1. HOLEXTWECL-182 HOLEXTW BLE: Overload Status is not being published when measurement is greater than 105%
    2. HOLEXTWECL-179 Wrench goes to standby also if the user is active on mobile App
    3. HOLEXTWECL-178 Configuration of counter option is not saved in nonvolatile memory if activated by App
    4. HOLEXTWECL-177 HOLEXTW BLE: DeviceMeasurementResult.StatusOfMeasurement Bit 3 is not set
    5. HOLEXTWECL-175 HOLEXTW: Deactivated Angle function: Angle mode can be activated via BLE
    6. HOLEXTWECL-174 HOLEXTW BLE: Publishing MeasurementCaseData
    7. HOLEXTWECL-173 HOLEXTW FW: Live value is not the same as Peak value after a re-adjustment (Calibrator SW) is done
    8. HOLEXTWECL-171 HOLEXTW FW: No voltage monitoring when "Battery Low" screen pops up
    9. HOLEXTWECL-170 HOLEXTW BLE: FW hangs after two times connectiong with iOS
   10. HOLEXTWECL-168 HOLEXTW FW: Correct Screens
   11. HOLEXTWECL-167 HOLEXTW BLE: Live Data Cycle too high
   12. HOLEXTWECL-166 HOLEXTW BLE: History file. No angle cases are saved. Double entries in history.
   13. HOLEXTWECL-165 HOLEXTW BLE: In angle mode data are not transmitted correctly to IOS or Android.
   14. HOLEXTWECL-164 HOLEXTW BLE measurement_sequence_number increased after a power cycle
   15. HOLEXTWECL-162 HOLEXTTW: APP_CONNECTION_ACTIVE_FLAG dissappears once  send button is pressed
   16. HOLEXTWECL-161 HOLEXTW FW: "Recalibration required" screen does not appear when the wrench is turned on
   17. HOLEXTWECL-156 HOLEXTW FW: Torque Triggering and Angle mode: It is possible to select a value that is not in the range
   18. HOLEXTWECL-108 HOLEXTW BLE: MeasurementCount in DeviceMeasurementResult is not increased
   19. HOLEXTWECL-95 HOLEXTW BLE: Battery load not shown correctly on PC

Holex V0.2.10:
    1. HOLEXTWECL-159 HOLEXTW FW: Overload Info - Indicating mode: Wrong visualization of direction of rotation
    2. HOLEXTWECL-158 HOLEXTW FW: Angle Mode in "in.lb" and "ft.lb" units: Incorrect Min and Max Angle Tolerance calculation
    3. HOLEXTWECL-157 HOLEXTW FW: "Battery Low" pop-ups screens are not correctly visualized at low voltage
    4. HOLEXTWECL-156 HOLEXTW FW: Torque Triggering and Angle mode: It is possible to select a value that is not in the range
    5. HOLEXTWECL-155 HOLEXTW FW: Not possible to turn on the wrench when USB cable is connected
    6. HOLEXTWECL-152 Measurement is possible if Traceability mode is activated and connected to wrong App/mobile/device
    7. HOLEXTWECL-146 HOLEXTW BLE: Correct Date and Time sent by HCT-App is acknowledged with INVALID_DATA and will not be taken over
    8. HOLEXTWECL-145 HOLEXTW BLE: Minimal dimming time and auto power off time not checked
    9. HOLEXTWECL-138 HOLEXTW FW: Last measured value when wrench turned off
   10. HOLEXTWECL-128 HOLEXTW FW: Dependencies of Connection Sub-Menu
   11. HOLEXTWECL-110 HOLEXTW FW: Screen blinks, flashes
   12. HOLEXTWECL-108 HOLEXTW BLE: MeasurementCount in DeviceMeasurementResult is not increased
   13. HOLEXTWECL-86 HOLEXTW FW: Minimize Angle Drift

Holex V0.2.9:
    1.HOLEXTWECL-149 HOLEXTW BLE: No measurement result data after measurement and no measurement control data after send-button!!
    2.HOLEXTWECL-148 HOLEXTW BLE: Activation of Traceability-Mode by App fails because of no Publish
    3.HOLEXTWECL-147 HOLEXTW BLE: No MeasurementControl after sequence counter reset
    4.HOLEXTWECL-136 HOLEXTW BLE. Traceability mode after reconnection still active
    5.HOLEXTWECL-12 HOLEXTW FW: Tare Action not performed

Holex V0.2.8:
    1. HOLEXTWECL-144 HOLEXTW BLE: If the Traceability Mode is established and the connection is lost, then the Warning screen must appear
    2. HOLEXTWECL-143 HOLEXTW FW: Charging screen blinks during a the charging when wrench is off
    3. HOLEXTWECL-142 HOLEXTW FW: V0.2.7 Update Problem
    4. HOLEXTWECL-140 HOLEXTW FW: When I switch OFF Bluetooth in Connections, TW hangs and can_t be recovered
    5. HOLEXTWECL-138 HOLEXTW FW: Last measured value when wrench turned off
    6. HOLEXTWECL-136 HOLEXTW BLE. Traceability mode after reconnection still active
    7. HOLEXTWECL-134 HOLEXTW BLE: Traceability Mode can be switched off with the wrong SessionID
    8. HOLEXTWECL-133 HOLEXTW BLE: DeviceMeasurementLimitsEffectiveLengthMax not preset
    9. HOLEXTWECL-130 HOLEX_TW BLE: Writing Administration Data returns INVALID_DATA (0x0B )
   10. HOLEXTWECL-129 HOLEXTW FW: Offset Torque when battery voltage is lower than 3,26V
   11. HOLEXTWECL-128 HOLEXTW FW: Dependencies of Connection Sub-Menu
   12. HOLEXTWECL-127 HOLEXTW BLE: BT-Reset takes 8 sec, can be shortened to 2.
   13. HOLEXTWECL-122 HOLEXTW FW: Main screen turns black after "Battery Low" is poped up and OK is pressed
   14. HOLEXTWECL-121 HOLEXTW BLE: Wrong Overload Status
   15. HOLEXTWECL-108 HOLEXTW BLE: MeasurementCount in DeviceMeasurementResult is not increased
   16. HOLEXTWECL-97 HOLEXTW BLE: TraceabilityMode Availability is set to off
   17. HOLEXTWECL-95 HOLEXTW BLE: Battery load not shown correctly on PC
   18. HOLEXTWECL-93 HOLEXTW BLE: SequenceCounter cannot be reset via BLE
   19. HOLEXTWECL-91 HOLEXTW FW: "Unit" selection for Torque Triggering and Angle mode
   20. HOLEXTWECL-78 APP-Connection is without function
   21. Avoid multiple Lic_Validate() check during power up to save boot up time when attached to PC.

Holex V0.2.7:
    1. Updrade to ble_proxy_lib v0.2.2.
    2. HOLEXTWECL-137 HOLEXTW BLE: After switch on I can read the Traceability Session ID, should be 0xFFFFFFFF
    3. HOLEXTWECL-135 HOLEXTW BLE: When publishing TracreabilityMode TraceabilityModeAvailable is also published
    4. HOLEXTWECL-134 HOLEXTW BLE: Traceability Mode can be switched off with the wrong SessionID
    5. HOLEXTWECL-131 HOLEXTW BLI: Flag "Measurement is a repetition" has to be cleared if measurement case configuration gets changed
    6. HOLEXTWECL-130 HOLEX_TW BLE: Writing Administration Data returns INVALID_DATA (0x0B )
    7. HOLEXTWECL-126 HOLEXTW: FW HID OFF --> HID Sub Setting inactive and grey
    8. HOLEXTWECL-125 HOLEXTW: FW Default Settings for Sign (HID)
    9. HOLEXTWECL-124 HOLEXTW BLE: Check values for date (over BLE) if it is an existing date
   10. HOLEXTWECL-123 HOLEXTW FW: V0.2.6 update problem
   11. HOLEXTWECL-121 HOLEXTW BLE: Wrong Overload Status
   12. HOLEXTWECL-119 HOLEXTW BLE: If Traceability mode is initialized and no connection established I still can perform screw actions and loose results
   13. HOLEXTWECL-118 HOLEXTW BLE: If indicating mode is active, no HID data is sent
   14. HOLEXTWECL-113 HOLEXTW FW: Angle mode not licenced
   15. HOLEXTWECL-111 HOLEXTW FW: Wrong screen visualization in when wrench is turned off
   16. HOLEXTWECL-110 HOLEXTW FW: Screen blinks, flashes
   17. HOLEXTWECL-106 HOLEXTW BLE: When new mode is created on Wrench, no MeasurementControl is sent
   18. HOLEXTWECL-88 HOLEXTW FW: Current Consumption according to the Brightness

Holex V0.2.6:
    1. HOLEXTWECL-12   HOLEXTW FW: Tare Action not performed            
    2. HOLEXTWECL-93   HOLEXTW BLE: SequenceCounter cannot be reset via BLE   
    3. HOLEXTWECL-104  HOLEXTW FW: Torque Triggering and Angle mode: Measurement 0,0Nm          
    4. HOLEXTWECL-107  HOLEXTW BLE: Repetition in Measurement Result Status    
    5. HOLEXTWECL-112  HOLEXTW FW: V0.2.5 update problem          
    6. HOLEXTWECL-114  HOLEXTW FW: Angle mode - Incorrect visualization of the angle measurement.                
    7. HOLEXTWECL-115  HOLEXTW FW: For DTW 12Nm - "Recalibration required" screen does not pop up from range 140% to 200% (16,8 to 24Nm)                
    8. HOLEXTWECL-116  HOLEXTW FW: INFO Screen "Versione"

Holex V0.2.5:
    1. HOLEXTWECL-13  :HOLEXTW FW: Live value is refreshed faster than Peak value.  
    2. HOLEXTWECL-29  :HOLEXTW FW: BT Reset does not disconnect connection to PC       
    3. HOLEXTWECL-39  :HOLEXTW FW: Last Measurement Screen Implementation       
    4. HOLEXTWECL-78  :APP-Connection is without function   
    5. HOLEXTWECL-80  :HOLEXTW FW: Overload Info: Incorrect visualization of measured values in CCW.       
    6. HOLEXTWECL-87  :HOLEXTW FW: Translation Table update
    7. HOLEXTWECL-88  :HOLEXTW FW: Current Consumption according to the Brightness
    8. HOLEXTWECL-90  :HOLEXTW FW: Angle mode: "Result" screen visualization error
    9. HOLEXTWECL-91  :HOLEXTW FW: "Unit" selection for Torque Triggering and Angle mode
   10. HOLEXTWECL-92  :HOLEXTW BLE: SequenceCounter in MeasurementControl is always 0
   11. HOLEXTWECL-93  :HOLEXTW BLE: SequenceCounter cannot be reset via BLE
   12. HOLEXTWECL-94  :HOLEXTW FW: Menu >> Connection >> QR code: Visualization error
   13. HOLEXTWECL-95  :HOLEXTW BLE: Battery load not shown correctly on PC
   14. HOLEXTWECL-96  :HOLEXTW FW: Headlines in capital letters
   15. HOLEXTWECL-97  :HOLEXTW BLE: TraceabilityMode Availability is set to off
   16. HOLEXTWECL-98  :HOLEXTW BLE: Reading the Traceability Mode via BLE when Mode is OFF
   17. HOLEXTWECL-99  :HOLEXTW BLE: When initializing the TraceabilityMode TW does not send the PublicMessage to show the Active State
   18. HOLEXTWECL-100 :Display turns off if brightness is set to 12%
   19. HOLEXTWECL-101 :HOLEXTW FW: Counter ON to OFF and ON again without reset of Counter
   20. HOLEXTWECL-102 :HOLEXTW FW: Upper symbols are not always refreshed
   21. HOLEXTWECL-103 :HOLEXTW FW: Battery voltage supervision in Background
   22. HOLEXTWECL-104 :HOLEXTW FW: Torque Triggering and Angle mode: Measurement 0,0Nm
   23. HOLEXTWECL-105 :HOLEXTW FW: Add Type of wrench in INFO screen
   24. HOLEXTWECL-106 :HOLEXTW BLE: When new mode is created on Wrench, no MeasurementControl is sent
   25. HOLEXTWECL-107 :HOLEXTW BLE: Repetition in Measurement Result Status
   26. HOLEXTWECL-109 :HOLEXTW FW: Menu >> Mode: Angle >> ... >> Target Angle: Error in the visualization

Holex V0.2.4:
    1. HOLEXTWECL-85 : HOLEXTW FW: "Result" and "Repeat" screens, visualization of measurment in CCW rotation for Torque Triggering and Angle mode
    2. HOLEXTWECL-82 : HOLEXTW FW: Menu >> Settings >> Measurement >> Evaluation time: Bug when B2 (<) is pressed.
    3 .HOLEXTWECL-81 : HOLEXTW FW: Menu >> Settings >> Measurement >> Effective Lenght
    4 .HOLEXTWECL-80 : Overload Info: Incorrect visualization of measured values in CCW.
    5 .HOLEXTWECL-79 : HOLEXTW FW: Indicating Mode: Incorrect screen visualization above 100% torque measurement
    6 .HOLEXTWECL-77 : Integrate Sequence Number in MeasurementControl
    7 .HOLEXTWECL-76 : Integrate Traceability Mode
    8 .HOLEXTWECL-75 : Mode is saved when sent from App but not activated after restart
    9 .HOLEXTWECL-74 : HOLEXTW BLE: Lower Tolerance is taken over with the wrong sign.
    10.HOLEXTWECL-72 : HOLEXTW FW: Menu >> Settings >> Display >> Brightness: Incorrect selection range
    11.HOLEXTWECL-63 : HOLEXTW FW: Angle triggering with effective length not same as default
    12.HOLEXTWECL-62 : HOLEXTW FW: Effective length
    13.HOLEXTWECL-40 : HOLEXTW FW: Implement aligned Battery symbols
    14.HOLEXTWECL-39 : HOLEXTW FW: Last Measurement Screen Implementation
    15.HOLEXTWECL-37 : HOLEXTW FW: Cut-Off Voltage of 3,00V is not implemented
    16.HOLEXTWECL-34 : HOLEXTW FW: "Calibration Required" screens never pops up after the wrench is overloaded.

Holex V0.2.3:
Holex V0.2.2:
1. Fixed following issues:
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-60
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-61
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-57
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-19


Holex V0.2.1:
1. Workaround for large memory usage in ble_proxy_core.c, it always cause hardfault when takes 10000 bytes:
    uint8_t resp_buffer[1024];   // <-- shrinked from 10000 to 1024
2. Updrade to ble_proxy_lib v0.1.9.
3. Fixed following issues:
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-8
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-9
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-43
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-44
https://hoffmann-group-digital.atlassian.net/browse/HOLEXTWECL-57



Holex V0.2.0:
1. Updrade to ble_proxy_lib v0.1.7.
Holex V0.1.4:
1. Updrade to ble_proxy_lib v0.1.6.
2. Enabled WrenchConfig [Update BT Firmware] by:
   a) BT_PROG on.
   b) BT_NRST off for 10ms.
   c) BT_NRST on.
   d) wait 50ms.
   e) BT_PROG off.

Holex V0.1.3:
1.[FA07]: Counter Option is restarting from zero after the tool is restarted.
2.[FC07]: Menu >> Mode >> Torque >> Indicating >> "Unit" ,Change "Unit" to "Start"
3.[FC11]: Last measured value screen (Button 1) Typo "Last measured vlaue"
4.[FC13]: Torque Triggering (Result)
    For OK Result and NOK Result:
    Screen on the bottom: Typo in "Send" --> " at the end
5.[FC20]: Menu >> Settings >> Display >> Standby
    - It is possible to select the Standby time from 00-99 min, with steps of 01 (despite the Standby time is from 0,5 min to 15 min with steps of 0,5).
6.[FC25]: - When Time Format is 12h, in the selection of TIME then the hours can´t be correctly set when pushing B4 (˅) --> hour does not decrease, it increases. 
    how it should be: B4(˅) should decrease the hour.
7.[FC26]: - Time Format: 24h --> It is possible to set 24:60, that is not correct. See figure beside
    - Time Format: 12h --> It is possible to set 12:60 am/pm , that is not correct.
8.[FC27]: - "Counter Reset" option is enabled when "Counter" is ON, and disabled when "Counter" is OFF --> OK, but
    - Counter Option: It is not possible to set ON/OFF correctly. See FF05
9.[FC28]: Menu >> Settings >> Measurement >> Counter
    - After the tool is turned off and turned on, the counter is reseted
10.[FC29]: Threshold from 50 - 99 %
11.[FC30]: Menu >> Settings >> Measurement >> Evaluation time
    - It is possible to select the Evaluation time from 00-99 sec, with steps of 01 (despite the Evaluation time is from 01 sec to 10 sec, with steps of 01).
12.[FC32]: Menu >> Settings >> System >> Master PW >> Confirm Password
    - In case the confirmed password is not the same as the selected password, there is a 5th position to select a number.
13.[FC33]: - Incorrect numeration when there no entry: 1/0
    How it should be: If there is no entry, then no number to be indicated in the bottom middle position of screen
14.[FD03]: - Problem still not solved. Target value color changes to white as soon as a measurement begins for Torque Triggering and Angle Mode.
15.[FE03]: The peak value shown is higher than the live value
16.[FF01]: When the measurement result is OK, the screen visualization is not correct
17.[FF04]: In "Min Tolerance" and "Max Tolerance" screens, the " ° " symbol is missing, as shown in the figure beside
18.[FF05]: Menu >> Settings >> Measurement >> Counter
    Counter is ON: Not possible to set to OFF by selecting "OFF" option. One must select again "ON".
    Counter is OFF: Not possible to set to ON by selecting "ON" option. One must select again "OFF".
19.[FF06]: Torque Triggering:
    Issue 1: In "Min Tolerance" and "Max Tolerance" screens, there is an error in the units (%). After selecting the tolerance values, the selection goes to the unit, see figures beside.
    Issue 2: After selecting "0 , 1 %". Then going back to change the decimals (" 1 ", then button B4 (˅) does not work
20.[FF07]: Screen Typos:
    Issue 1: Menu >> "Cancel" instead of "cancel"
21.[FF08]: Menu >> Settings >> System >> Master PWD Despite Master PWD is enabled, the access to the menu is possible.
22.[FF09]: Torque Indicating Mode: Issue 1: "not calibrated" dissapears when a measurement starts, despite the measurement value is in the not calibrated range.
23.[FF10]: Check sound of the buzzer. Check the resonance frequency of the buzzer.
    Should have the same sound level as Garant Wrench. The sound level of Holex is far too low (not usable for our customers working in loud environment)
24.[FF11]: Menu >> Connection >> QR code
    After the QR code is shown, when B1 or B4 is pressed, and then B2 is pressed, the time to go back to the connection menu is too much
25.[FF12]: Turn ON time last more than 2 seconds. The time and behavior should be the same as Garant
26.[FF14]: Torque Triggering:
    - After a successful measurement, the visualization of the last measurement value shows an incorrect result
27.[FF16]: In all modes (Torque Indicating, Torque Triggering and Angle) --> Counter is enabled
    The counter always disappears as soon a measurement is performed. 
    Counter should not dissapears during a measurement.
28.[FF18]: In all modes (Torque Indicating, Torque Triggering and Angle)
    - Typo in Peak. It should always be "Peak: " (Peak,two points and space) and then the value
29.[FF21]: In German Menu: The seperating of Fügemome-nt is wrong. Please seperate Füge-moment
30.[FF22]: In German Menu: The line FÜGEMOMENT. is on the upper side of the line not in the middle.
31.[FF23]: In German Menu: The seperating of Drehrichtu-ng is wrong. Please seperate Deh-richtung
32.[FF24]: In German the wrong english expression appears, not the german one. This happens only in the indicating mode. Expected is Letzter Messwert.
33.[FF25]: Factory reset is not taken over directly after reset done. It needs to restart the wrench to get in factory setting status. How it should be: like Garant, after factory reset the factory setting shall directly be shown without restart of wrench
34.[FF26]: Factory reset screen: In German the english text is displayed.
35.[FF27]: Overload Info: In German: The line ÜBERLAST INFO. is on the upper side of the line not in the middle.
36.[FF28]: not calibrated: 
    When no torque applied: "not calibrated" not to be shown
    When torque applied and below 20% load: "not calibrated" to be shown in white color
    When torque applied and equal or above 20% load: "not calibrated" not to be shown
37.[FF29]: When wrench off and loading:
    Status 1: when battery not fully loaded then screen Charging-07 to be shown
    Status 2: when battery fully loaded then screen Charging-06 to be shown
38. Enable HID output.



Holex V0.1.2:

[Change]: Starting screen Holex Logo
[Add]:“not calibrated” sign on measurement screen
[FW]
Please use Holex TFT To test FCXX Issue
1. [FC01]: Indicating Mode: Not possible to visualize the direction of rotation (“↺” or “↻”) during the measurement.
2. [FC02]: Counter Option is restarting from zero after the tool is restarted
3. [FC03]: On DTW only torque indicating and triggering can be activated, it seems that angle function is not available, but it should. (Activation by license key will come later)
4. [FC05]: When the wrench is turned on, and Tare action is not successfull, " Tare not successfull, repeat?" screen pops up. After the next Tare action is done, the home screen is not correctly updated (tittle "TARE" is on home screen)
5. [FC06]: Angle Mode:Not possible to select Angle mode
6. [FC07]: Indicating Mode: In the left bottom right corner (related to Button 3), it should be named "Start" and not "Unit >> (Follow inVision show "Menu")
7. [FC09]: Idicating Mode: When the counter is enabled, its position is not the same one as in the specification. >> (Follow inVision ,please check about that) 
8. [FC10]: Idicating Mode:When the counter is enabled, it is reseted after the tool is turned off and turned on.
9. [FC11]: Last measured value screen (Button 1) Typo "Last measured vlaue"
10.[FC12]: Torque Triggering:Target Value: It is possible to set the minimum limt under 20% of nominal value.
11.[FC13]: Torque Triggering (Result) For OK Result and NOK Result: Screen on the bottom: Typo in "Send" --> " at the end
12.[FC14]: Menu >> Connection - "Button Transfer": B3 does not react
13.[FC19]: Menu >> Settings >> Display >> Brightness - It is possible to select the brightness from 00-100% (despite the brightness of the screes is from 12-100%)
14.[FC20]: Menu >> Settings >> Display >> Standby- It is possible to select the Standby time from 00-99 min, with steps of 01 (despite the Standby time is from 0,5 min to 15 min with steps of 0,5). >> (Follow inVision Standby time from 01-99 min with steps of 1)
15.[FC21]: Menu >> Settings >> Standby - Standby time is not correctly updated 
16.[FC22]: Menu >> Settings >> Display >> Dimming - It is possible to select the Dimming time from 00-99 sec, with steps of 01 (despite the Dimming time is from 30 sec to 300 sec, with steps of 30).>> (Follow inVision Dimming time from 01-99 sec with steps of 1)
17.[FC23]: Menu >> Settings >> Date - Day and month configuration error
18.[FC24]: Menu >> Settings >> Display >> Date - Year selection button (˅) B4 does not work
19.[FC25]: Menu >> Settings >> Display >>Time - Selection of the hour decimal is not working correctly, button (˅)
20.[FC26]: Menu >> Settings >> Display >> Time - Selection of the minutes units is not correct (69 minutes)
21.[FC27]: Menu >> Settings >> Measurement >> Counter When this option is "OFF", the "Counter Reset" option is available
22.[FC28]: Menu >> Settings >> Measurement >> Counter - After the tool is turned off and turned on, the counter is reseted 
23.[FC29]: Menu >> Settings >> Measurement >> Threshold - It is possible to select the threshold from 00 to 100%. It must be possible to select from 50% to 100%.
24.[FC30]: Menu >> Settings >> Measurement >> Evaluation time - It is possible to select the Evaluation time from 00-99 sec, with steps of 01 (despite the Evaluation time is from 0,5 sec to 10 sec, with steps of 01).>> (Follow inVision Evaluation time from 01-99 sec with steps of 1)
25.[FC31]: Menu >> Settings >> Measurement >> Effective Length - Selection of the decimal is not working correctly, button (˅) B4
26.[FC32]: Menu >> Settings >> System >> Master PW >> Confirm Password - In case the confirmed password is not the same as the selected password, there is a 5th position to select a number. 
27.[FC33]: Menu >> Settings >> System >> Master PW >> Overload Info
           - Incorrect numeration XX/0, if you press B4 then the numeration increases
           - It is possible to select empty spaces. See figure.
28.[FC34]: Wrench Overloaded:
           - When the wrench is overloaded, it is not possible to unlock it using the CALIBRATOR SW. The tool is blocked.

29.[FC36]: Autoroll with B1 (˄) and B4 (˅) to select an option is not working 
30.[FD01]: Default rotation should be "clockwise" and not "counter-clockwise"
31.[FD02]: When screwcase not successful and the user clicks repeat, then it is not needed to push Send button (button 5). But when user chose to not repeat, then Send button must be pressed. This behaviour is now implemented in the wrong arrangement
32.[FD03]: Target value to be indicated in grey as long as the wrench is within "not calibrated range". When in calibrated range then value to be shown in white (same as the actual value and same as for Garant)
33.[FD04]: Angle measurement not correct. 
           Issue 1: The tolerance must be set in degree and not in % 
           Issue 2: The angle measurements starts already before snug point is reached
           Issue 3: Angle value is increasing very fast even if no rotation at all
           Issue 4: Torque value is as well shown in green or red but should always stay in neutral colour for angle triggering


[BT]
1.[BC01]: Setpoint data tolerance value lower should be negativ [-9.9..-0.1]%, but are positive !! 
          Also angle value tolerances
2.[BC02]: Setpoint tolerance values are not taken over if a new set point data is updated and sended from App to Wrench. It seems that if we read back the set point data, the min and max tolerance values are cero
3.[BC03]: Angle Mode configured through the App. After a failed measurement, the upper and lower tolerance values are written to cero and sended incorrectly to the app as new setpoint data
4.[BC04]: It is not possible to deactivate the Master PW from the App. Wrench is not updating correctly the deactivation of the PW in the wrench
5.[BC08]: Master PWD is disabled in App, but wrench is not updated to this status
6.[BE04]: Specialy after a few changes of settings BLE connection is lost and wrench is frozen
7.[BE05]: Evaluation time setting dos not work properly sometimes- Set to 10s -> set to 1s -> still 10s on reload
8.[BE06]: Master PWD switch on is working but switch off not

Holex V0.1.1:
1. Add USB MSC device.
2. Add overload counter save option that could not be clear.
3. Fix torque/angle freeze issue.

Holex V0.1.0:
1. Ported to Holex PCB.

Holex V0.0.7:
1. Power off BT complete in early boot.
2. Power on BT depends on BT enabled, and reset BT 10ms.

Holex V0.0.6:
1. Master Password automatically requested with v0.0.5, why? It should not be requested if not set manually.
   Please do factory reset after update firmware.
2. Sometimes Setpoint values from App to Wrench are not taken over by Wrench  (e.g. if Mode is changed in App from torque triggering to Indicating or Angle-Measurement).
3. In some situation if (maybe wrong) button is pressed then wrench application crashes. à Deactivate/ Ignore the not needed buttons. Can you describe shortly which buttons from the Garant will be used by Holex-FW for which function.
4. Initial configuration data: If an internal configuration package has been sent from Tool-Controller to BLE-Controller, then Tool-SW has to wait until acknowledge from BLE controller comes before sending the next command. (This is different to our test-program) If you do so, you do not need to wait 100 ms before sending the next command, you just wait for the acknowledge. Acknowledge timeout should be 1s.
   Set the maximum acknowledge time to 1S.
5. Fixed BT icon always solid bug.
6. Update to BLE_PROXY_LIB Version 0.0.5. Call SetSecurity_BLE_SEC_LEGACYSEC_BOND() insted of PresetSecurityStructure().

Holex V0.0.5:
1. Add BT_CTS/MCU_RTS check before send data.
2. Fixed HID output.
3. Update to BLE_PROXY_LIB Version 0.0.4.
4. Implement DeviceSetpointUpdateCb(), DeviceAdministrationUpdateCb(), DeviceApperianceSetupUpdateCb().

Holex V0.0.4:
1. Synchronized ModuleBLEConnectionState structure into tool app.
2. Fixed live torque/angle output, mobile App received live values but BLE hangs later.
3. Synchronized DeviceHistory structure into tool app.
4. Synchronized DeviceScrewCaseConfiguration structure into tool app.
5. Synchronized DeviceAdministration, DeviceCommunicationSetup, DeviceApperianceSetup structure into tool app.

Holex V0.0.3:
1. Upgrade to BLE_PROXY V0.0.2.
2. Tool Application send commands just after BLE-Module power on response.

Holex V0.02:
1.Added following to compiler.h for Keil compiler, the “ModuleAdvertising” Length changed from 0x54 to 0x50.
#elif defined(__ARMCC_VERSION)
               #define BEGIN_PACKED_STRUCT_DEFINITIONS _Pragma("pack(1)")
               #define END_PACKED_STRUCT_DEFINITIONS _Pragma("pack()")

2. The MCU CTS is set to 0.
3. The BLE response after 1500+ ms.(Page 1 of PPT).
4. There seems not LDS notification connection update from BLE to TOOL-MCU.
